{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["CÁLCULO DE ESFORÇOS DE LINHA DE","BD","FATOR DE QUEDA","CARGA RUPT CABO DE AÇO_CIMAF"],"not_rendered":{"charts":0,"images":25,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CÁLCULO DE ESFORÇOS DE LINHA DE","index":0,"n_rows":81,"n_cols":29,"rows_kept":81,"cut":false,"hidden":false,"merged":[[76,0,76,1],[40,11,40,14],[49,4,49,6],[14,0,14,1],[0,0,0,1],[37,0,37,1]]}
["DADOS"]
["Restrição de Movimentação?","Não"]
["Peso do corpo(P) + ferramentas + roupas",100,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100]
["Vão(L) - Distância entre apoios total",20]
["Número de Vãos",1]
["Vão(L) - Distância entre apoios",20]
["Diâmetro do cabo (dc)",9.52]
["Força de ruptura do cabo (fu)",6100]
["Número de pessoas (n)",1]
["Comprimento do talabarte (a)",1.4]
["Comprimento do abs. estendido (b)",1.1000000000000001]
["Uso de trava-quedas retrátil (A1)",0.9]
["Espaço de frenagem trava-quedas retrátil (B1)",1.9]
["Distância posição recolhida a posição de trabalho (b1)",1]
["CÁLCULOS"]
["Flecha (%)",{"$f":"IF(B2=\"Sim\",0.01,0.03)","v":0.03}]
["Comprimento do cabo x% (L1)",{"$f":"(1+(0.666666*((B19/(B6*1000/2))^2)))*B6*1000","v":20047.999951999998}]
["Dl alongamento cabo parabólico(ΔL)",{"$f":"(B36*B17)/(9500*0.396*$B$7^2)","v":132.26936057267315}]
["Flecha inicial parabólica (montagem) (f1)",{"$f":"B6*1000*B16","v":600}]
["Flecha inicial cabo reto (f2)",{"$f":"SQRT((B17*0.5)^2-(B6*0.5*1000)^2)","v":693.23554355499334},"1 vão","1 vão +"]
["Flecha total carga dinâmica (f3)",{"$f":"IF(B5=1,SQRT((((B17+B18)/2)^2)-((B6*1000*0.5)^2)),SQRT((((B18*B5*0.5)+((0.5*B6*1000)))^2)-((0.5*1000*B6)^2)))","v":1345.6661480436303},{"$f":"SQRT((B17/2+B18/2)^2-(B6*1000/2)^2)","v":1345.6661480436303},{"$f":"SQRT((((B18*B5*0.5)+((0.5*B6*1000)))^2)-((0.5*1000*B6)^2))","v":1151.9841151957428},"mm"]
["Distância de frenagem",{"$f":"B21-B20","v":652.43060448863696}]
["Carga corpo (P)",{"$f":"IF(B2=\"Não\",600+((B9-1)*B3*1.2),B9*100)","v":600}]
["Força no cabo (T1)",{"$f":"(B23*((B17/2)+(B18/2)))/(B21)/2","v":2249.4735423691104}]
["Força admissível (Fadm) do cabo tabela fabricante coef seg 2 ou mais",{"$f":"B8/2*0.8","v":2440}]
["Número de pessoas (n)",{"$f":"B9","v":1}]
["Hmin cabo/piso – talabarte (ZLQ1)",{"$f":"B10+B11+(B21/1000)+1.8+1","v":6.6456661480436301}]
["Hmin cabo/piso – trava-quedas (ZLQ 2 )",{"$f":"B12+(B21/1000)+1.8+1","v":5.0456661480436305}]
["Dist. piso trab/piso abaixo p/ trava-quedas (Hp)",{"$f":"B21/1000-B19/1000+B13-B14+1","v":2.6456661480436301}]
["Coeficiente de utilização do cabo - sempre menor que 100%",{"$f":"B24/B25","v":0.92191538621684854}]
["Fator de serviço do cabo",{"$f":"(B25*2)/B24","v":2.1693964868155153}]
["Informe o fator de queda",1]
["Status de calibração",{"$f":"IF(AND(B35<1,B35>-1),\"CALIBRADO\",\"CORRIGIR\")","v":"CALIBRADO"}]
["Status resistencia do cabo de aço",{"$f":"IF(OR(AND(B2=\"Não\",B31>=2),(AND(B2=\"Sim\",B31>=3))),\"APROVADO\",\"REPROVADO\")","v":"APROVADO"}]
["VARÁVEL DE SIMULAÇÃO",{"$f":"B36-B24","v":-3.5379389373701997E-7}]
["FORÇA CABO – ITERAÇÃO",2249.4735420153165]
[]
["ANÁLISE SEM ABSORVEDOR"]
["Angula â",{"$f":"DEGREES(ATAN(C21/(B6*0.5*1000)))","v":7.6640596749453538}]
["Força max Fx",{"$f":"B24*COS(RADIANS(B39))","v":2229.379110384466}]
["Força  max Fy",{"$f":"B24*SIN(RADIANS(B39))","v":300}]
["Força max possível F angula a",{"$f":"B24","v":2249.4735423691104}]
["Mx",{"$f":"B40*(B50/1000)","v":557.3447775961165}]
["My",{"$f":"B41*(B50/1000)","v":75}]
["Momento máximo ângulo a",{"$f":"B42*(B50/1000)","v":562.3683855922776}]
[]
[]
[null,null,null,null,"https://www.gulin.com.br/"]
[]
["h = altura do ancoragem",250]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["distancia entre centros",180]
[]
[]
["Força dos parafusos *d = Momento do pilarete"]
["Fp=(Mx/d)/2 parafusos",{"$f":"B43*0.5/(B70/1000)","v":1548.1799377669904}]
["Fp em cada parafuso",{"$f":"B74*10/1000","v":15.481799377669905}]
[]
["ANÁLISE COM ABSORVEDOR LINHA DE VIDA"]
["Força max possível F angula a",1400]
["Momento máximo ângulo a",{"$f":"B78*(B50/1000)","v":350}]
["Fp em cada parafuso",{"$f":"B79*0.5/(B70/1000)","v":972.22222222222229}]
["Fp em cada parafuso",{"$f":"B80*10/1000","v":9.7222222222222232}]

{"sheet":"BD","index":1,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Restrição de Movimentação"]
["Sim"]
["Não"]

{"sheet":"FATOR DE QUEDA","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"CARGA RUPT CABO DE AÇO_CIMAF","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}